Aberration resistant axial localization using a self-imaging of vortices. Opt. Express, 23, 15316?15331 (2015201520152015).