Stable a-CSi:H films with a wide range of modulus of elasticity and low internal stress. Surface and Coatings Technology, 459, 129147 (2023202320232023).

Experimental analysis of microhardness changes of subsurface areas affected by WEDM. Proceedings of the Institution of Mechanical Engineers, Part E: Journal of Process Mechanical Engineering, 236, 1979-1991 (2022202220222022).

Surface topography affects the nanoindentation data. Thin Solid Films, 745, 139105 (2022202220222022).